;   88x Analog Stream driver Tuner Install Information File For Win2000, WinXP, MCE
;
;       
;
;   Copyright (c) 2005-2006 DVB-DTV Technology Inc.
;   All Rights Reserved.
;
;

[Version]
signature="$CHICAGO$"
Class=Media
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider="DTV-DVB"
DriverVer=08/25/2006,1.0.2.9
CatalogFile.NTx86=88XAStream.cat
CatalogFile.NTAMD64=AMD64\88XAStream.cat
CatalogFile.NTIA64=IA64\88XAStream.cat

[Manufacturer]
"DTV-DVB"=DTV-DVB, NTx86, NTAMD64, NTIA64

[SourceDisksNames]
1="DVB-DTV PCI Analog Stream Driver",,

[SourceDisksNames.AMD64]
1="DVB-DTV PCI Analog Stream Driver",88xAStream.inf, , \AMD64

[SourceDisksNames.IA64]
1="DVB-DTV PCI Analog Stream Driver",88xAStream.inf, , \IA64

[SourceDisksFiles]
88xAStream.sys=1

[DTV-DVB.NTx86]
; MB86A16 tuner & tda9887(all standard)
%CX23880.videoMoto%=CX23880.MB86A16,PCI\VEN_14F1&DEV_8800&SUBSYS_00231822
%CX23880.videoMoto%=CX23880.MB86A16,PCI\VEN_14F1&DEV_8800&SUBSYS_117A153B

[DTV-DVB.NTAMD64]
; MB86A16 tuner & tda9887(all standard)
%CX23880.videoMoto%=CX23880.MB86A16,PCI\VEN_14F1&DEV_8800&SUBSYS_00231822
%CX23880.videoMoto%=CX23880.MB86A16,PCI\VEN_14F1&DEV_8800&SUBSYS_117A153B

[DTV-DVB.NTIA64]
; MB86A16 tuner & tda9887(all standard)
%CX23880.videoMoto%=CX23880.MB86A16,PCI\VEN_14F1&DEV_8800&SUBSYS_00231822
%CX23880.videoMoto%=CX23880.MB86A16,PCI\VEN_14F1&DEV_8800&SUBSYS_117A153B

[DestinationDirs]
CX23880.CopyDrivers=10,system32\drivers
CX23880.CopyFilters=11

[CX23880.CopyDrivers]
88xAStream.sys

[CX23880.CopyFilters]
; none for now


[CX23880.MB86A16]
Include=    ks.inf, kscaptur.inf, ksfilter.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT,MSPCLOCK.Installation
AddReg=     CX23880.AddReg,MB86A16.AddReg
CopyFiles=  CX23880.CopyDrivers,CX23880.CopyFilters

[CX23880.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,88xAStream.sys
HKR,,OkToHibernate,3,01
HKR,,PageOutWhenUnopened,3,00
HKR,,DontSuspendIfStreamsAreRunning,3,01
HKR,"DriverData","XBarInPin0",0x00010001, 0x03,0x00,0x00,0x00
HKR,"DriverData","XBarInPin1",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","XBarInPin2",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData","XBarInPin3",0x00010001, 0x00,0x10,0x00,0x00
HKR,"DriverData","XTal0",0x00010001, 0x1c, 0x00, 0x00, 0x00
HKR,"DriverData","XTal1",0x00010001, 0x23, 0x00, 0x00, 0x00
HKR,"DriverData","BobMode",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","VolumeLevelNegdB",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","UseExternalVPRES",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","UseI2SAsClock",0x00010001, 0x00, 0x00, 0x00, 0x00


[MB86A16.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ColorKillEnable",0x00010001, 0x01,0x00,0x00,0x00
; Country code is USA = 1 
HKR,"DriverData","WWAudioCountryCode",0x00010001, 0x01,0x00,0x00,0x00 
HKR,"ENUM\Device1",pnpid,,"cxtune.VEN_14F1.MB86A16" 
HKR,"ENUM\Device2",pnpid,,"cx88xbar.VEN_14F1.MB86A16"

[VideoCapture]
AddReg=VideoCapture.AddReg

;[VideoTvAudio]
;AddReg=VideoTvAudio.AddReg

[VideoCapture.AddReg]
HKR,,CLSID,,{17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%CX23880.friendly%

[VideoTvAudio.AddReg]
;HKR,,CLSID,,{71F96462-78F3-11d0-A18C-00A0C9118956}
;HKR,,FriendlyName,,%CX23880.friendly2%

[CX23880.MB86A16.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture,
;AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoTvAudio,

[CX23880.MB86A16.Services]
AddService = CX23880,0x00000002,CX23880.ServiceInstall

[CX23880.ServiceInstall]
DisplayName   = %CX23880.video%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_AUTO_START%
ErrorControl  = %SERVICE_ERROR_NORMAL%
ServiceBinary = %10%\system32\drivers\88xAStream.sys

[Strings]
CX23880.video               = "DTV-DVB 1027 Analog Video Capture"
CX23880.friendly            = "DTV-DVB 1027 Analog Video Capture"
CX23880.friendly2           = "DTV_DVB 1027 TvAudio"
CX23880.videoMoto	        = "DTV-DVB 1027 Analog Video Capture"
;RunOnce                    = "SOFTWARE\Microsoft\Windows\CurrentVersion\RunOnce"
SERVICE_KERNEL_DRIVER       = 1
SERVICE_AUTO_START          = 2
SERVICE_ERROR_NORMAL        = 1


