;****************************************************************************************
;
; rt2500usb.inf
;
;   This installation script supports Windows 98,Me,2000 & XP for the
;   Belkin 54g USB Network Adapter.
;
;   Copyright (c)2004, Belkin Corporation., All Rights Reserved
;
;****************************************************************************************

[Version]
Signature       = "$Chicago$"
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %Provider%
Compatible      = 1
DriverVer       = 07/15/2004, 1.02.00.0000
CatalogFile    = rt2500usb.CAT            ;for WHQL certified

[ControlFlags]
;***********BELKIN 802.11g board  ***********
;ExcludeFromSelect = USB\VID_050D&PID_7050

[Manufacturer]
%BELKIN%        = BELKIN

[BELKIN]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%BELKIN.DeviceDesc% =       BELKIN.ndi,             USB\VID_050D&PID_7050

;*******************************************************************************************
; Windows 9X specific entries
;*******************************************************************************************

[BELKIN.ndi]
AddReg                  = Common.reg, BELKIN.ndi.reg
CopyFiles               = win9x.CopyFiles

;*******************************************************************************************
; NT specific entries
;*******************************************************************************************

[BELKIN.ndi.NT]
AddReg                  = Common.reg, BELKIN.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

; NT services sections
[BELKIN.ndi.NT.Services]
AddService              = bkn50USB, 2, BELKIN.Service, common.EventLog

;*******************************************************************************************
; common regs for NT and W9x
;*******************************************************************************************


[Common.reg]
;*******************************************************************************************
; System Level Property

;
; Current Profile
;
HKR, ,                    CurProfile,      0,""
HKR, Default,             CurProfile,      0,""

;
; Radio On/Off
;
HKR, ,                            Radio,           0, "0"
HKR, NDI\params\Radio,            ParamDesc,       0, "Radio On/Off"
HKR, NDI\params\Radio,            type,            0, "enum"
HKR, NDI\params\Radio,            default,         0, "0"
HKR, NDI\params\Radio\enum,       1,               0, "Disable"
HKR, NDI\params\Radio\enum,       0,               0, "Enable"

;
; Auto Reconnect Mode
;
HKR, ,                                  AutoReconnect,      0, "1"
HKR, NDI\params\AutoReconnect,          ParamDesc,          0, "Auto Reconnect Mode"
HKR, NDI\params\AutoReconnect,          type,               0, "enum"
HKR, NDI\params\AutoReconnect,          default,            0, "1"
HKR, NDI\params\AutoReconnect\enum,     0,                  0, "Disable"
HKR, NDI\params\AutoReconnect\enum,     1,                  0, "Enable"

;
; Show Hidden SSID in Site Survey Page
;
HKR, ,                                  ShowHiddenSSID,     0, "0"   ; 0=disable(default), 1=enable

;
; Select Config Utility
;
HKR, ,                                  ConfigSelect,       0, "0"   ;0=RaConfig, 1=ZeroConfig

;
; Country Region 
;
HKR, ,                                  CountryRegion,      0, "2"
;HKR, NDI\params\CountryRegion,         ParamDesc,          0, "Country Region"
;HKR, NDI\params\CountryRegion,         type,               0, "enum"
;HKR, NDI\params\CountryRegion,         default,            0, ""
;HKR, NDI\params\CountryRegion\enum,    0,                  0, "FCC (Channel 1 - 11)"
;HKR, NDI\params\CountryRegion\enum,    1,                  0, "IC (Channel 1 - 11)"
;HKR, NDI\params\CountryRegion\enum,    2,                  0, "ETSI (Channel 1 - 13)"
;HKR, NDI\params\CountryRegion\enum,    3,                  0, "Spain (Channel 10 - 11)"
;HKR, NDI\params\CountryRegion\enum,    4,                  0, "France (Channel 10 - 13)"
;HKR, NDI\params\CountryRegion\enum,    5,                  0, "MKK (Channel 14)"
;HKR, NDI\params\CountryRegion\enum,    6,                  0, "MKK1 (Channel 1 - 14)"
;HKR, NDI\params\CountryRegion\enum,    7,                  0, "Israel (Channel 3 - 9)"

;*******************************************************************************************
; Advance Page

;
; WirelessMode
;
HKR, ,                            WirelessMode,    0, "0"

;
; Enable TX Burst
;
HKR, ,                            TXBurst,         0, "0"

;
; Use Short Slot Time
;
HKR, ,                            ShortSlot,       0, "0"

;
; Use Turbo rate
;
HKR, ,                            TurboRate,       0, "0"

;
; Use Ofdm rate in adhoc mode
;
HKR, ,                            AdhocOfdm,       0, "0"

;
; Use BG Protection
;
HKR, ,                            BGProtection,    0, "0"

;
; Vendor Description
;
HKR, ,                            VendorDesc,      0, %VENDOR_DESC_DEF_STR%
HKR, Default,                     VendorDesc,      0, %VENDOR_DESC_DEF_STR%

;*******************************************************************************************
; Profile

;
; SSID
;
HKR, ,                            SSID,            0, %SSID_DEF_STR%
HKR, Default,                     SSID,            0, %SSID_DEF_STR%
HKR, NDI\params\SSID,             ParamDesc,       0, "SSID"
HKR, NDI\params\SSID,             type,            0, "edit"
HKR, NDI\params\SSID,             limitText,       0, "32"
HKR, NDI\params\SSID,             default,         0, %SSID_DEF_STR%

;
; Network Type
;
HKR, ,                            NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, Default,                     NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType,      ParamDesc,       0, "Network Type"
HKR, NDI\params\NetworkType,      type,            0, "enum"
HKR, NDI\params\NetworkType,      default,         0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType\enum, 0,               0, "802.11 Ad Hoc"
HKR, NDI\params\NetworkType\enum, 1,               0, "Infrastructure"

;
; Channel
;
HKR, ,                            Channel,         0, %CHANNEL%
HKR, Default,                     Channel,         0, %CHANNEL%


;*******************************************************************************************
; System Configuration Page

;
; Local Administration MAC Network Address
;
HKR, ,                            NetworkAddress,  0, ""
HKR, Default,                     NetworkAddress,  0, ""
HKR, NDI\params\NetworkAddress,   ParamDesc,       0, "Local Administration MAC Network Address"
HKR, NDI\params\NetworkAddress,   type,            0, "edit"
HKR, NDI\params\NetworkAddress,   limitText,       0, "12"
HKR, NDI\params\NetworkAddress,   default,         0, ""

;
; Power Saving Mode
;
HKR, ,                            PSMode,          0, "0"
HKR, Default,                     PSMode,          0, "0"
HKR, NDI\params\PSMode,           ParamDesc,       0, "Power Saving Mode"
HKR, NDI\params\PSMode,           type,            0, "enum"
HKR, NDI\params\PSMode,           default,         0, "0"
HKR, NDI\params\PSMode\enum,      0,               0, "CAM (Constantly Awake Mode)"
HKR, NDI\params\PSMode\enum,      1,               0, "Max_PSP (Max Power Savings)"
HKR, NDI\params\PSMode\enum,      2,               0, "Fast_PSP (Power Save Mode)"

;
; CAM when AC Power
;
HKR, ,                            ACPowerCam,      0, "0"
HKR, Default,                     ACPowerCam,      0, "0"
HKR, NDI\params\ACPowerCam,       ParamDesc,       0, "CAM when AC Power"
HKR, NDI\params\ACPowerCam,       type,            0, "enum"
HKR, NDI\params\ACPowerCam,       default,         0, "0"
HKR, NDI\params\ACPowerCam\enum,  0,               0, "Disable"
HKR, NDI\params\ACPowerCam\enum,  1,               0, "Enable"

;
; Preamble Type
;
HKR, ,                            PreambleType,    0, "0"
HKR, Default,                     PreambleType,    0, "0"

;
; RTS Threshold
;
HKR, ,                            RTSThresh,       0, "2347"
HKR, Default,                     RTSThresh,       0, "2347"
HKR, NDI\params\RTSThresh,        ParamDesc,       0, "RTS Threshold"
HKR, NDI\params\RTSThresh,        type,            0, "int"
HKR, Ndi\params\RTSThresh,        default,         0, "2347"
HKR, NDI\params\RTSThresh,        min,             0, "0"
HKR, NDI\params\RTSThresh,        max,             0, "2347"
HKR, NDI\params\RTSThresh,        step,            0, "32"
HKR, NDI\params\RTSThresh,        optional,        0, "0"

;
; Fragment Threshold
;
HKR, ,                            FragThresh,      0, "2346"
HKR, Default,                     FragThresh,      0, "2346"
HKR, NDI\params\FragThresh,       ParamDesc,       0, "Fragment Threshold"
HKR, NDI\params\FragThresh,       type,            0, "int"
HKR, Ndi\params\FragThresh,       default,         0, "2346"
HKR, NDI\params\FragThresh,       min,             0, "256"
HKR, NDI\params\FragThresh,       max,             0, "2346"
HKR, NDI\params\FragThresh,       step,            0, "32"
HKR, NDI\params\FragThresh,       optional,        0, "0"

;*******************************************************************************************
; Authentication & Security Page

;
; Authentication Type
;
HKR, ,                AuthenType,      0, "0" ; Open System
HKR, Default,         AuthenType,      0, "0"

;
; Encryption
;
HKR, ,                Encryption,      0, "1" ; Disable
HKR, Default,         Encryption,      0, "1"

;
; WEP Keys Length
;
HKR, ,                WEPKeyLen,       0, "0"
HKR, Default,         WEPKeyLen,       0, "0"

;
; WEP Key to use
;
HKR, ,                WEPKeyUse,       0,"1"
HKR, Default,         WEPKeyUse,       0,"1"

;
; WEP Key1
;
HKR, ,                WEPKey1,         0,""
HKR, Default,         WEPKey1,         0,""

;
; WEP Key2
;
HKR, ,                WEPKey2,         0,""
HKR, Default,         WEPKey2,         0,""

;
; WEP Key3
;
HKR, ,                WEPKey3,         0,""
HKR, Default,         WEPKey3,         0,""

;
; WEP Key4
;
HKR, ,                WEPKey4,         0,""
HKR, Default,         WEPKey4,         0,""


;*******************************************************************************************
; APConfig use
;

;
; WPA Group-Key ReKey Interval
;
HKR, ,                RekeyInterval,   0, "60"

;
; WPA Group-Key ReKey Method
;
HKR, ,                RekeyMethod,     0, "0"


[BELKIN.ndi.reg]
HKR, ,                            NTMPDriver,       0, rt25u98.sys
HKR, Ndi,                         DeviceID,         0, "USB\VID_148F&PID_2570"

HKR, ,                            BusType,          0, 15
HKR, NDI,                         CardType,         0, "PNP"

HKR, ,                            RunningWin9X,     0, "1"
HKR, ,                            DevLoader,        0, "*ndis"
HKR, ,                            DeviceVxDs,       0, "rt25u98.sys"
HKR, ,                            EnumPropPages,    0, "netdi.dll,EnumPropPages"

HKR, Ndi\Interfaces,              DefUpper,         0, "ndis3"
HKR, Ndi\Interfaces,              DefLower,         0, "ethernet"
HKR, Ndi\Interfaces,              UpperRange,       0, "ndis3"
HKR, Ndi\Interfaces,              LowerRange,       0, "ethernet"

HKR, NDIS,                        LogDriverName,    0, "rt25u98.sys"
HKR, NDIS,                        MajorNdisVersion, 1, 03
HKR, NDIS,                        MinorNdisVersion, 1, 0A

;
; Interfaces
;
;
; Install sections
;HKR,Ndi\Install,ndis3,,"rt25u98.install"

;*******************************************************************************************
; DestinationDirs
;*******************************************************************************************

[DestinationDirs]
NT.CopyFiles            = 12    ; system32\drivers subdirectory on NT
win9x.CopyFiles         = 11    ; system32 subdirectory on win9x

[NT.CopyFiles]
rt2500usb.sys                   ; NT Installation

[win9x.CopyFiles]
rt25u98.sys                     ; Win9x Installation

[SourceDisksNames]
1                       = %INSTALL_DISK_STR%,,,

[SourceDisksFiles] 
rt2500usb.sys           = 1
rt25u98.sys             = 1


;*******************************************************************************************
; NT specific
;*******************************************************************************************
[BELKIN.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "bkn50USB"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "ethernet"

[BELKIN.Service]
DisplayName                 = %BELKIN.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt2500usb.sys
LoadOrderGroup              = NDIS

[common.EventLog]
AddReg=common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\rt2500usb.sys"
HKR, , TypesSupported,   0x00010001, 7


;*******************************************************************************************
; Strings
;*******************************************************************************************
[strings]
Provider                    = "BELKIN"
BELKIN                      = "Belkin Corporation"

BELKIN.DeviceDesc           = "Belkin 54Mbps Wireless USB Network Adapter"
INSTALL_DISK_STR            = "Belkin 54Mbps Wireless USB Installation Disk"
BELKIN.Service.DispName     = "Belkin 54Mbps Wireless USB Network Adapter"
;
; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
SSID_DEF_STR                = ""
VENDOR_DESC_DEF_STR         = ""
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "1"
