; RDT172LM.inf
; Setup information file for NMV LCD Monitor RDT172LM
;
; Copyright 2003, NEC-MITSUBISHI ELECTRIC VISUAL SYSTEMS CORPORATION
;-------------------------------------------------
[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%MITSUBISHI%
CatalogFile=RDT172LM.cat
DriverVer=11/18/2003,3.11.0018.0853

[ControlFlags]
ExcludeFromSelect.nt=Monitor\MEL4675
ExcludeFromSelect.nt=Monitor\MEL4676

[DestinationDirs]
DefaultDestDir = 11
RDT172LM.CopyFiles = 23

[SourceDisksNames]
1=%Disk1%,,,

[SourceDisksFiles]
RDT172LM.icm=1

[Manufacturer]
%MITSUBISHI%=MITSUBISHI

[MITSUBISHI]
%RDT172LM-A%=RDT172LM-A.Install, Monitor\MEL4675
%RDT172LM-D%=RDT172LM-D.Install, Monitor\MEL4676

; Install Sections
;-------------------------------------------------
[RDT172LM-A.Install]
DelReg=DEL_CURRENT_REG
AddReg=RDT172LM-A.AddReg, 1280, DPMS
CopyFiles=RDT172LM.CopyFiles

[RDT172LM-D.Install]
DelReg=DEL_CURRENT_REG
AddReg=RDT172LM-D.AddReg, 1280, DPMS
CopyFiles=RDT172LM.CopyFiles

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

; Pre-defined AddReg sections
[1280]
HKR,,MaxResolution,,"1280,1024"

[DPMS]
HKR,,DPMS,,1

; Model AddReg sections
[RDT172LM-A.AddReg]
HKR,"MODES\1280,1024",Mode1,,"31.0-83.0,56.0-75.0,+,+"
HKR,,ICMProfile,0,"RDT172LM.icm"

[RDT172LM-D.AddReg]
HKR,"MODES\1280,1024",Mode1,,"31.0-70.0,56.0-75.0,+,+"
HKR,,ICMProfile,0,"RDT172LM.icm"

[RDT172LM.CopyFiles]
RDT172LM.icm

[Strings]
MITSUBISHI="NEC-MITSUBISHI ELECTRIC VISUAL SYSTEMS"
RDT172LM-A="MITSUBISHI TFT RDT172LM(Analog)"
RDT172LM-D="MITSUBISHI TFT RDT172LM(Digital)"
Disk1="Mitsubishi Display Monitor Installation Disk"
