;
; TDAUSBPT.SYS setup INF file ver 2.3.0.0
;
[Version]
Signature="$CHICAGO$"
Class=USB
ClassGUID={36FC9E60-C465-11CF-8056-444553540000}
Provider=%PANASONIC%
DriverVer=03/02/2010,2.3.0.0
; Copyright 2004 by Panasonic System Networks Co., Ltd.
CatalogFile.NTAMD64 = TDAUSBPTamd64.cat

; =================== Table of content =========================
[SourceDisksNames]
1=%KXTDAUSB.SrcDesc%,,,

[SourceDisksFiles]
TDAUSBPT.sys = 1
KXTDAUSB.Dll = 1

[Manufacturer]
%MfgName%=PANASONIC, NTamd64

[PANASONIC]
%USB\VID_04DA&PID_1681&MI_00.DeviceDesc%=KXTDAUSB.Dev, USB\VID_04DA&PID_1681&MI_00

[PANASONIC.NTamd64]
%USB\VID_04DA&PID_1681&MI_00.DeviceDesc%=KXTDAUSB.Dev, USB\VID_04DA&PID_1681&MI_00

[PreCopySection]
HKR,,NoSetupUI,,1

[DestinationDirs]
KXTDAUSB.Files.Ext=10,System32\Drivers
KXTDAUSB.Files.Dll=16425 ; N.Ishida for windows(WOW64)

[KXTDAUSB.Dev]
CopyFiles=KXTDAUSB.Files.Ext, KXTDAUSB.Files.Dll
AddReg=KXTDAUSB.AddReg

[KXTDAUSB.Dev.NT]
CopyFiles=KXTDAUSB.Files.Ext, KXTDAUSB.Files.Dll
AddReg=KXTDAUSB.AddReg.NT

[KXTDAUSB.Dev.NT.Services]
Addservice = TDAUSBPT, 0x00000002, KXTDAUSB.AddService

[KXTDAUSB.AddService]
DisplayName    = %KXTDAUSB.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\TDAUSBPT.sys
;ServiceBinary  = %12%\TDAUSBPT.sys
LoadOrderGroup = Base

[KXTDAUSB.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,TDAUSBPT.sys
HKLM,"Software\Panasonic\KX-TDA USB",LogDir,,%24%\"Progra~1\Panasonic\KX-TDA USB"
HKLM,"Software\Panasonic\KX-TDA USB",Wakeup,0x00000001,01
HKLM,"Software\Microsoft\Windows\CurrentVersion\RunOnce",CreateLogDirectory,,"RUNDLL32.EXE KXTDAUSB.DLL,CreateLogDirectory"

[KXTDAUSB.AddReg.NT]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,TDAUSBPT.sys
HKLM,"Software\Wow6432Node\Panasonic\KX-TDA USB",LogDir,,%16426%\"Panasonic\KX-TDA USB"
HKLM,"Software\Wow6432Node\Panasonic\KX-TDA USB",Wakeup,0x00000001,01
HKLM,"Software\Wow6432Node\Microsoft\Windows\CurrentVersion\RunOnce",CreateLogDirectory,,"RUNDLL32.EXE KXTDAUSB.DLL,CreateLogDirectory"

[KXTDAUSB.Files.Ext]
TDAUSBPT.sys

[KXTDAUSB.Files.Dll]
KXTDAUSB.dll

;---------------------------------------------------------------;

[Strings]
PANASONIC="PANASONIC"
MfgName="Panasonic"
KXTDAUSB.SvcDesc="Panasonic KX-TDA USB PT Unit driver"
USB\VID_04DA&PID_1681&MI_00.DeviceDesc="Panasonic KX-TDA USB PT Unit driver"
KXTDAUSB.SrcDesc="Panasonic KX-TDA USB driver Installation Disks"
