; Windows 2000/XP Virtual Serial Port Setup File
; Copyright (c) 2002-2006 AnyDATA Corporated
; Manufacturer: AnyDATA Corporated
;
; This INF file installs a virtual COM port on a 64-bit Windows system.

[Version]
signature  = "$WINDOWS NT$"
Class      = Ports
Provider   = %ANYDATA%
ClassGuid  = {4D36E978-E325-11CE-BFC1-08002BE10318}
CatalogFile.ntia64=adser_ia64.cat
CatalogFile.ntamd64=adser_amd64.cat
DriverVer  = 12/21/2006,2.0.3.7

[ControlFlags]
ExcludeFromSelect = *

[SourceDisksNames]
1=%DISKNAME%,,1

[SourceDisksFiles]
adusbser.sys=1

[Manufacturer]
%ANYDATA% = AnyDataSerialPort, NTia64, NTamd64

[AnyDataSerialPort]

[AnyDataSerialPort.NTia64]
%AnyDATADevice011% = AnyDATAportInstall00, USB\VID_16D5&PID_6001&MI_01
%AnyDATADevice021% = AnyDATAportInstall00, USB\VID_16D5&PID_6002&MI_01
%AnyDATADevice022% = AnyDATAportInstall00, USB\VID_16D5&PID_6002&MI_02
%AnyDATADevice031% = AnyDATAportInstall00, USB\VID_16D5&PID_6003&MI_01
%AnyDATADevice032% = AnyDATAportInstall00, USB\VID_16D5&PID_6003&MI_02

%AnyDATADevice011_65% = AnyDATAportInstall00, USB\VID_16D5&PID_6501&MI_01
%AnyDATADevice021_65% = AnyDATAportInstall00, USB\VID_16D5&PID_6502&MI_01
%AnyDATADevice022_65% = AnyDATAportInstall00, USB\VID_16D5&PID_6502&MI_02
%AnyDATADevice031_65% = AnyDATAportInstall00, USB\VID_16D5&PID_6503&MI_01
%AnyDATADevice032_65% = AnyDATAportInstall00, USB\VID_16D5&PID_6503&MI_02
%AnyDATADevice041_65% = AnyDATAportInstall00, USB\VID_16D5&PID_6504&MI_01
%AnyDATADevice042_65% = AnyDATAportInstall00, USB\VID_16D5&PID_6504&MI_02
%AnyDATADevice043_65% = AnyDATAportInstall00, USB\VID_16D5&PID_6504&MI_03

%AnyDATADevice011_68% = AnyDATAportInstall00, USB\VID_16D5&PID_6801&MI_01
%AnyDATADevice021_68% = AnyDATAportInstall00, USB\VID_16D5&PID_6802&MI_01
%AnyDATADevice022_68% = AnyDATAportInstall00, USB\VID_16D5&PID_6802&MI_02
%AnyDATADevice031_68% = AnyDATAportInstall00, USB\VID_16D5&PID_6803&MI_01
%AnyDATADevice032_68% = AnyDATAportInstall00, USB\VID_16D5&PID_6803&MI_02
%AnyDATADevice041_68% = AnyDATAportInstall00, USB\VID_16D5&PID_6804&MI_01
%AnyDATADevice042_68% = AnyDATAportInstall00, USB\VID_16D5&PID_6804&MI_02
%AnyDATADevice043_68% = AnyDATAportInstall00, USB\VID_16D5&PID_6804&MI_03

%AnyDATADevice011_62% = AnyDATAportInstall00, USB\VID_16D5&PID_6201&MI_01
%AnyDATADevice021_62% = AnyDATAportInstall00, USB\VID_16D5&PID_6202&MI_01
%AnyDATADevice022_62% = AnyDATAportInstall00, USB\VID_16D5&PID_6202&MI_02
%AnyDATADevice031_62% = AnyDATAportInstall00, USB\VID_16D5&PID_6203&MI_01
%AnyDATADevice032_62% = AnyDATAportInstall00, USB\VID_16D5&PID_6203&MI_02
%AnyDATADevice041_62% = AnyDATAportInstall00, USB\VID_16D5&PID_6204&MI_01
%AnyDATADevice042_62% = AnyDATAportInstall00, USB\VID_16D5&PID_6204&MI_02
%AnyDATADevice043_62% = AnyDATAportInstall00, USB\VID_16D5&PID_6204&MI_03

[AnyDataSerialPort.NTamd64]
%AnyDATADevice011% = AnyDATAportInstall00, USB\VID_16D5&PID_6001&MI_01
%AnyDATADevice021% = AnyDATAportInstall00, USB\VID_16D5&PID_6002&MI_01
%AnyDATADevice022% = AnyDATAportInstall00, USB\VID_16D5&PID_6002&MI_02
%AnyDATADevice031% = AnyDATAportInstall00, USB\VID_16D5&PID_6003&MI_01
%AnyDATADevice032% = AnyDATAportInstall00, USB\VID_16D5&PID_6003&MI_02

%AnyDATADevice011_65% = AnyDATAportInstall00, USB\VID_16D5&PID_6501&MI_01
%AnyDATADevice021_65% = AnyDATAportInstall00, USB\VID_16D5&PID_6502&MI_01
%AnyDATADevice022_65% = AnyDATAportInstall00, USB\VID_16D5&PID_6502&MI_02
%AnyDATADevice031_65% = AnyDATAportInstall00, USB\VID_16D5&PID_6503&MI_01
%AnyDATADevice032_65% = AnyDATAportInstall00, USB\VID_16D5&PID_6503&MI_02
%AnyDATADevice041_65% = AnyDATAportInstall00, USB\VID_16D5&PID_6504&MI_01
%AnyDATADevice042_65% = AnyDATAportInstall00, USB\VID_16D5&PID_6504&MI_02
%AnyDATADevice043_65% = AnyDATAportInstall00, USB\VID_16D5&PID_6504&MI_03

%AnyDATADevice011_68% = AnyDATAportInstall00, USB\VID_16D5&PID_6801&MI_01
%AnyDATADevice021_68% = AnyDATAportInstall00, USB\VID_16D5&PID_6802&MI_01
%AnyDATADevice022_68% = AnyDATAportInstall00, USB\VID_16D5&PID_6802&MI_02
%AnyDATADevice031_68% = AnyDATAportInstall00, USB\VID_16D5&PID_6803&MI_01
%AnyDATADevice032_68% = AnyDATAportInstall00, USB\VID_16D5&PID_6803&MI_02
%AnyDATADevice041_68% = AnyDATAportInstall00, USB\VID_16D5&PID_6804&MI_01
%AnyDATADevice042_68% = AnyDATAportInstall00, USB\VID_16D5&PID_6804&MI_02
%AnyDATADevice043_68% = AnyDATAportInstall00, USB\VID_16D5&PID_6804&MI_03

%AnyDATADevice011_62% = AnyDATAportInstall00, USB\VID_16D5&PID_6201&MI_01
%AnyDATADevice021_62% = AnyDATAportInstall00, USB\VID_16D5&PID_6202&MI_01
%AnyDATADevice022_62% = AnyDATAportInstall00, USB\VID_16D5&PID_6202&MI_02
%AnyDATADevice031_62% = AnyDATAportInstall00, USB\VID_16D5&PID_6203&MI_01
%AnyDATADevice032_62% = AnyDATAportInstall00, USB\VID_16D5&PID_6203&MI_02
%AnyDATADevice041_62% = AnyDATAportInstall00, USB\VID_16D5&PID_6204&MI_01
%AnyDATADevice042_62% = AnyDATAportInstall00, USB\VID_16D5&PID_6204&MI_02
%AnyDATADevice043_62% = AnyDATAportInstall00, USB\VID_16D5&PID_6204&MI_03

[AnyDATAportInstall00.NTia64]
CopyFiles=ADUsbDriverFiles
AddReg = All00, AddReg

[AnyDATAportInstall00.NTamd64]
CopyFiles=ADUsbDriverFiles
AddReg = All00, AddReg

[ADUsbDriverFiles]
adusbser.sys

[DestinationDirs]
DefaultDestDir = 12

[AnyDATAportInstall00.NTia64.Services]
AddService=adusbser,  0x00000002, AD_USBSerialService

[AnyDATAportInstall00.NTamd64.Services]
AddService=adusbser,  0x00000002, AD_USBSerialService

[AD_USBSerialService]
DisplayName   = %ADUSBSER%
ServiceType   = 1
StartType     = 3
ErrorControl  = 1
ServiceBinary = %12%\adusbser.sys

[All00]
HKR,,NTMPDriver,,adusbser.sys

[AddReg]
HKR,,PortSubClass,1,01
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"
HKLM,SYSTEM\CurrentControlSet\Services\adusbser,QCDriverSelectiveSuspendIdleTime,0x10001,30

[Strings]
ANYDATA   = "AnyDATA Corporation"
AnyDATADevice011 = "AnyDATA CDMA USB Serial Device (PID 6001)"
AnyDATADevice021 = "AnyDATA CDMA USB Serial 1 (DIAG) Device (PID 6002)"
AnyDATADevice022 = "AnyDATA CDMA USB Serial 2 (NMEA) Device (PID 6002)"
AnyDATADevice031 = "AnyDATA CDMA USB Serial 1 (DIAG) Device (PID 6003)"
AnyDATADevice032 = "AnyDATA CDMA USB Serial 2 (AUX) Device (PID 6003)"

AnyDATADevice011_65 = "AnyDATA CDMA USB Serial Device (PID 6501)"
AnyDATADevice021_65 = "AnyDATA CDMA USB Serial 1 (DIAG) Device (PID 6502)"
AnyDATADevice022_65 = "AnyDATA CDMA USB Serial 2 (NMEA) Device (PID 6502)"
AnyDATADevice031_65 = "AnyDATA CDMA USB Serial 1 (DIAG) Device (PID 6503)"
AnyDATADevice032_65 = "AnyDATA CDMA USB Serial 2 (AUX) Device (PID 6503)"
AnyDATADevice041_65 = "AnyDATA CDMA USB Serial 1 (DIAG) Device (PID 6504)"
AnyDATADevice042_65 = "AnyDATA CDMA USB Serial 2 (NMEA) Device (PID 6504)"
AnyDATADevice043_65 = "AnyDATA CDMA USB Serial 3 (AUX) Device (PID 6504)"

AnyDATADevice011_68 = "AnyDATA CDMA USB Serial Device (PID 6801)"
AnyDATADevice021_68 = "AnyDATA CDMA USB Serial 1 (DIAG) Device (PID 6802)"
AnyDATADevice022_68 = "AnyDATA CDMA USB Serial 2 (NMEA) Device (PID 6802)"
AnyDATADevice031_68 = "AnyDATA CDMA USB Serial 1 (DIAG) Device (PID 6803)"
AnyDATADevice032_68 = "AnyDATA CDMA USB Serial 2 (AUX) Device (PID 6803)"
AnyDATADevice041_68 = "AnyDATA CDMA USB Serial 1 (DIAG) Device (PID 6804)"
AnyDATADevice042_68 = "AnyDATA CDMA USB Serial 2 (NMEA) Device (PID 6804)"
AnyDATADevice043_68 = "AnyDATA CDMA USB Serial 3 (AUX) Device (PID 6804)"

AnyDATADevice011_62 = "AnyDATA WCDMA USB Serial Device (PID 6201)"
AnyDATADevice021_62 = "AnyDATA WCDMA USB Serial 1 (DIAG) Device (PID 6202)"
AnyDATADevice022_62 = "AnyDATA WCDMA USB Serial 2 (NMEA) Device (PID 6202)"
AnyDATADevice031_62 = "AnyDATA WCDMA USB Serial 1 (DIAG) Device (PID 6203)"
AnyDATADevice032_62 = "AnyDATA WCDMA USB Serial 2 (AUX) Device (PID 6203)"
AnyDATADevice041_62 = "AnyDATA WCDMA USB Serial 1 (DIAG) Device (PID 6204)"
AnyDATADevice042_62 = "AnyDATA WCDMA USB Serial 2 (NMEA) Device (PID 6204)"
AnyDATADevice043_62 = "AnyDATA WCDMA USB Serial 3 (AUX) Device (PID 6204)"

ADUSBSER = "AnyDATA USB Device for Legacy Serial Communication"
DISKNAME = "AnyDATA USB Modem Driver installation"
