;+-----------------------------------------------------------------------+
;| Device name    : Belkin Wireless G USB Adapter                        |
;| Platform	  : Microsoft Windows XP 64 bit    		         |
;| Host interface : USB                                                  |
;|                                                                       |
;| Copyright (c) 2000-2007 Belkin Technology Corporation.                |
;| All Rights Reserved.                                                  |
;+-----------------------------------------------------------------------+

;-------------------------------------------------------------------------
[Version]
Signature		= "$Chicago$"
Compatible		= 1
Class			= Net
ClassGUID		= {4d36e972-e325-11ce-bfc1-08002be10318}
Provider		= %INFProvider%
CatalogFile		= BLKWGU.cat			; for WHQL certified
DriverVer		= 02/08/2007,6.3.2.16


[Manufacturer]
%Manufacturer%	= Belkin, ntamd64


[ControlFlags]

[Belkin.ntamd64]
;DisplayName              Section           Hardware ID
;-----------              -------           --------------------------
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ntamd64, USB\VID_050D&PID_705C


[ZD1211BXP50U.ntamd64]
Characteristics = 0x84
BusType         = 15
AddReg		= ZD1211B_WinXP.reg, ZD1211B_Common.reg
CopyFiles       = ZD1211B.CopyFilesXP64

[ZD1211BXP50U.ntamd64.Services]
AddService = %CustomServiceName%, 2, ZD1211BU_NT.Service, ZD1211BU.EventLog

[ZD1211B_WinXP.reg]
; Interfaces Info
HKR,NDI\Interfaces,   UpperRange,         0, "ndis5"
HKR,NDI\Interfaces,   LowerRange,         0, "ethernet"
HKR,NDI,              Service,            0, %CustomServiceName%(%Manufacturer%)
HKR,,                 VendorDesc,         0, %VendorDesc%

[ZD1211B.CopyFilesXP64]
BLKWGU.sys,BLKWGU64.sys,,2

;*********************************************************************
;   Microsoft Windows 2000/XP Common Section
;*********************************************************************
;---------- 5.0 volt ----------
[ZD1211BU_NT.Service]
DisplayName     = %ZD1211BU.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\%DriverFileName%		; %12%\%DriverFileName%
LoadOrderGroup  = NDIS


;*********************************************************************
;   Microsoft Windows ME/2000/XP Common Section
;*********************************************************************
;---------- 5.0 volt ----------
[ZD1211BU.EventLog]
Addreg = ZD1211BU.AddEventLog.reg

[ZD1211BU.AddEventLog.reg]
HKR,,                               EventMessageFile,  0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR,,                               TypesSupported,    0x00010001, 7


;*********************************************************************
;   Destination Directories
;*********************************************************************
[DestinationDirs]
ZD1211B.CopyFilesXP64	= 12			; system32\drivers subdirectory on Win XP


[SourceDisksNames]
1=%DISKNAME%,,,


[SourceDisksFiles]
BLKWGU64.sys = 1


;******************************************************************************
[ZD1211B_Common.reg]
HKR, Ndi\params\NumRfd,         ParamDesc,  	0, "%ReceiveFrameDescriptors%"
HKR, Ndi\params\NumRfd,         default,    	0, "32"
HKR, Ndi\params\NumRfd,         min,        	0, "1"
HKR, Ndi\params\NumRfd,         max,        	0, "00001024"
HKR, Ndi\params\NumRfd,         step,       	0, "1"
HKR, Ndi\params\NumRfd,         Base,       	0, "10"
HKR, Ndi\params\NumRfd,         type,       	0, "int"
HKR, Ndi\params\NumRfd,         flag, 		1, 20,00,00,00

HKR, Ndi\params\NumTcb,         ParamDesc,  	0, "%TransmitControlBlocks%"
HKR, Ndi\params\NumTcb,         default,    	0, "32"
HKR, Ndi\params\NumTcb,         min,        	0, "1"
HKR, Ndi\params\NumTcb,         max,        	0, "00000064"
HKR, Ndi\params\NumTcb,         step,       	0, "1"
HKR, Ndi\params\NumTcb,         Base,       	0, "10"
HKR, Ndi\params\NumTcb,         type,		0, "int"
HKR, Ndi\params\NumTcb,         flag,		1, 20,00,00,00

HKR, Ndi\params\NumCoalesce,    ParamDesc,  	0, "%CoalesceBuffers%"
HKR, Ndi\params\NumCoalesce,    default,    	0, "128"
HKR, Ndi\params\NumCoalesce,    min,        	0, "1"
HKR, Ndi\params\NumCoalesce,    max,        	0, "00000128"
HKR, Ndi\params\NumCoalesce,    step,       	0, "1"
HKR, Ndi\params\NumCoalesce,    Base,       	0, "10"
HKR, Ndi\params\NumCoalesce,    type,       	0, "int"
HKR, Ndi\params\NumCoalesce,    flag, 		1, 20,00,00,00

HKR, Ndi\params\RTSCTSThreshold,    ParamDesc,  	0, "%RTSCTS%"
HKR, Ndi\params\RTSCTSThreshold,    default,    	0, "2347"
HKR, Ndi\params\RTSCTSThreshold,    min,        	0, "0"
HKR, Ndi\params\RTSCTSThreshold,    max,        	0, "2347"
HKR, Ndi\params\RTSCTSThreshold,    step,       	0, "1"
HKR, Ndi\params\RTSCTSThreshold,    Base,       	0, "10"
HKR, Ndi\params\RTSCTSThreshold,    type,       	0, "int"
HKR, Ndi\params\RTSCTSThreshold,    flag, 		1, 20,00,00,00

HKR, Ndi\params\FragmentThreshold,    ParamDesc,  	0, "%Fragment%"
HKR, Ndi\params\FragmentThreshold,    default,    	0, "2346"
HKR, Ndi\params\FragmentThreshold,    min,        	0, "256"
HKR, Ndi\params\FragmentThreshold,    max,        	0, "2346"
HKR, Ndi\params\FragmentThreshold,    step,       	0, "1"
HKR, Ndi\params\FragmentThreshold,    Base,       	0, "10"
HKR, Ndi\params\FragmentThreshold,    type,       	0, "int"
HKR, Ndi\params\FragmentThreshold,    flag, 		1, 20,00,00,00

HKR,,                           	PreambleMode,   0, "0"
HKR,NDI\params\PreambleMode,    	ParamDesc,      0, "PreambleMode"
HKR,NDI\params\PreambleMode,       	type,           0, "enum"
HKR,NDI\params\PreambleMode,           	flag,           1, 30,00,00,00
HKR,Ndi\params\PreambleMode,           	default,        0, "3"
HKR,NDI\params\PreambleMode\enum,      	1,              0, "Long"
HKR,NDI\params\PreambleMode\enum,      	2,              0, "Short"
HKR,NDI\params\PreambleMode\enum,      	3,              0, "Auto"

HKR,,                           	IBSS_G_Mode,    0, "0"
HKR,NDI\params\IBSS_G_Mode,    	        ParamDesc,      0, "IBSS_G_Mode"
HKR,NDI\params\IBSS_G_Mode,       	type,           0, "enum"
HKR,NDI\params\IBSS_G_Mode,           	flag,           1, 30,00,00,00
HKR,Ndi\params\IBSS_G_Mode,           	default,        0, "0"
HKR,NDI\params\IBSS_G_Mode\enum,      	0,              0, "Disable"
HKR,NDI\params\IBSS_G_Mode\enum,      	1,              0, "Enable"

HKR,,                           	IBSS_PureG_Mode,0, "0"
HKR,NDI\params\IBSS_PureG_Mode,    	ParamDesc,      0, "IBSS_PureG_Mode"
HKR,NDI\params\IBSS_PureG_Mode,       	type,           0, "enum"
HKR,NDI\params\IBSS_PureG_Mode,         flag,           1, 30,00,00,00
HKR,Ndi\params\IBSS_PureG_Mode,         default,        0, "0"
HKR,NDI\params\IBSS_PureG_Mode\enum,    0,              0, "Disable"
HKR,NDI\params\IBSS_PureG_Mode\enum,    1,              0, "Enable"

HKR,,                           	             Use_G_Mode_in_Usb1.1,0, "0"
HKR,NDI\params\Use_G_Mode_in_Usb1.1,    	     ParamDesc,      0, "Use_G_Mode_in_Usb1.1"
HKR,NDI\params\Use_G_Mode_in_Usb1.1,             type,           0, "enum"
HKR,NDI\params\Use_G_Mode_in_Usb1.1,             flag,           1, 30,00,00,00
HKR,Ndi\params\Use_G_Mode_in_Usb1.1,             default,        0, "0"
HKR,NDI\params\Use_G_Mode_in_Usb1.1\enum,        0,              0, "Disable"
HKR,NDI\params\Use_G_Mode_in_Usb1.1\enum,        1,              0, "Enable"

HKR,,                           	PSPXLinkMode,   0, "0"
HKR,NDI\params\PSPXLinkMode,    	        ParamDesc,      0, "PSPXLinkMode"
HKR,NDI\params\PSPXLinkMode,       	type,           0, "enum"
HKR,NDI\params\PSPXLinkMode,           	flag,           1, 30,00,00,00
HKR,Ndi\params\PSPXLinkMode,           	default,        0, "0"
HKR,NDI\params\PSPXLinkMode\enum,      	0,              0, "Disable"
HKR,NDI\params\PSPXLinkMode\enum,      	1,              0, "Enable"

HKR,,                           	QosTagPolicy,   0, "0"
HKR,NDI\params\QosTagPolicy,    	ParamDesc,      0, "QosTagPolicy"
HKR,NDI\params\QosTagPolicy,       	type,           0, "enum"
HKR,NDI\params\QosTagPolicy,           	flag,           1, 30,00,00,00
HKR,Ndi\params\QosTagPolicy,           	default,        0, "0"
HKR,NDI\params\QosTagPolicy\enum,      	0,              0, "Auto"
HKR,NDI\params\QosTagPolicy\enum,      	1,              0, "802.1Q Tag"
HKR,NDI\params\QosTagPolicy\enum,      	2,              0, "DSCP Tag"

HKR,,                           	WMMQosSupport,   0, "0"
HKR,NDI\params\WMMQosSupport,    	        ParamDesc,      0, "WMMQosSupport"
HKR,NDI\params\WMMQosSupport,       	type,           0, "enum"
HKR,NDI\params\WMMQosSupport,           	flag,           1, 30,00,00,00
HKR,Ndi\params\WMMQosSupport,           	default,        0, "0"
HKR,NDI\params\WMMQosSupport\enum,      	0,              0, "Disable"
HKR,NDI\params\WMMQosSupport\enum,      	1,              0, "Enable"

HKR,,                           PSMode,    	0, "0"
HKR,NDI\params\PSMode,          ParamDesc,      0, "PSMode"
HKR,NDI\params\PSMode,       	type,           0, "enum"
HKR,NDI\params\PSMode,         	flag,           1, 30,00,00,00
HKR,Ndi\params\PSMode,         	default,        0, "0"
HKR,NDI\params\PSMode\enum,    	0,              0, "Disable"
HKR,NDI\params\PSMode\enum,    	1,              0, "Enable"

HKR,,                           PHY_A_6M_Setpoint_Value,	0x10001, 0x28
HKR,,                           PHY_A_6M_CR128_Value,	0x10001, 0x17
HKR,,                           PHY_A_1dBm_Value,	0x10001, 0x08

;HKR,,                           FirmwareName,	0, %FirmwareFileName%
HKR,,                           EnableAntennaDiversity, 0, "0"
HKR,,                           DefaultAntenna, 0, "0"
HKR,,                           DefaultWirelessMode, 0, "0"


;*********************************************************************
[Strings]
INFProvider	= "Belkin"
Manufacturer	= "Belkin"

DISKNAME	= "Belkin Wireless G USB Network Adapter Installation Disk"

DriverFileName	= "BLKWGU.sys"
InterfaceType	= "USB"
CardType	= "PNP"
VendorDesc	= "Belkin Wireless G USB Network Adapter"
CustomServiceName = "BLKWGU"

ZD1211B_50U_DESC = "Belkin Wireless G USB Network Adapter"
ZD1211B_50U_PNP  = "USB\VID_050D&PID_705C"

ReceiveFrameDescriptors = "ReceiveFrameDescriptors"
TransmitControlBlocks = "TransmitControlBlocks"
CoalesceBuffers = "CoalesceBuffers"
RTSCTS = "RTSCTSThreshold"
Fragment = "FragmentThreshold"

ZD1211BU.Service.DispName 	= "Belkin Wireless G USB Network Adapter"
